Type: Dynamic coil type

Frequency response: 50Hz -16.5KHz

Directional shape: heart-shaped directionality

Output impedance: 300 Ω/600 Ω

Sensitivity: At 1 kHz, open circuit voltage -54.5 dB/Pa (1.85 mV)

Polarity: The positive pressure on the diaphragm can generate a positive voltage on pin 2 relative to pin 3

Line length: 5 meters